goMoto 3.3 (Early 2020 – Present)
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· Colours: Red and White
· Power: 1000W and 2000W models
· Top speed: 25 km/h and 45 km/h models
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General information
60V 45Ah (5 x 12V 45Ah lead-acid)
This is new model, and the only bigger change is motor axle’s wormgear and radio. If you cannot fix the differential gear, you might need to order whole new rear axle. Difference between old and new model is the motor axle’s wormgear, old one has gear with diameter of 24mm and new one 28mm. That is also why you need matching rear axle (differential is integrated). Always measure the wormgear before ordering anything.
If you see radio with screws on top plate corners right under the windscreen, you are holding old type goMoto 3.3.
Technical specifications
	Length
	2260 mm

	Width
	1160 mm

	Height
	1510 mm

	Wheelbase
	1700 mm

	Seat height
	520 mm from ground level, 320 mm from floor level

	Weight (including the batteries)
	240 kg

	Top speed
	25 km/h / 45 km/h

	Motors
	1000W or 1500W

	Brakes
	Hydraulic disc brakes

	Battery capacity
	2,7kWh = 60V 45Ah (5 x 12V 45Ah)

	Battery type
	Lead-acid VRLA

	Battery pack weight
	66 kg (5 x 13,2 kg)

	Range
	Up to 50 km

	Charging time
	Up to 12 hours, depending on the initial charge level of the batteries

	Maximum load
	150,5 kg

	Tyre size
	Front = 130/60R13 | Rear = 135/70R12

	Vehicle category
	L2e-P

	Number of seats
	2

	Seatbelt
	Yes

	Maximum torque of the motor
	48 N.m continuous

	Maximum hill-starting ability at the
maximum load
	8% slope

	Available colors
	Red and white
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