Technical data
	F02

	Maximum design speed 
	100km/h

	Dimension

	Full length 
	1954mm

	Full width 
	703mm

	Full height 
	1280mm

	Wheel Base
	1325mm

	Seat height 
	795mm

	Min Ground Clearance
	141mm

	Curb weight of whole vehicle 
	143kg

	

	Type
	Centrally-mounted wheel rim and permanent magnet synchronous motor 

	Rated bus voltage 
	72V

	Rated power/peak power 
	4kW/10kW

	Rated speed
	4KW/715±15rpm

	Rated torque 
	53N.m/715±15rpm

	Reduction ratio
	6.7

	Motor lubricating oil capacity 
	API GL-4 SAE 85W-9090mL

	Charger 

	Input Voltage
	180 Vac~240 Vac

	Rated Frequency
	50Hz〜60Hz

	Charging current 
	10A（900W）

	Power Battery (single) 

	Battery Type
	Ternary lithium battery 

	Nominal capacity 
	40Ah x 2 pcs = 80Ah

	Nominal Voltage 
	72 V

	Transmission

	Transmission mode
	Synchronous belt+aluminium pulley 

	Drive system 
	Motor Drive 

	Chassis 

	Tyre size 
	Front wheel 110/80-14 

	
	Rear wheel 130/70-13 

	Rim specification 
	Front wheel 2.50MTX14

	
	Rear wheel 3.50MTX13

	Electrical Installations 

	Headlight
	High beam LEDX6
Low beam  LEDX4
Front position lamp LEDX20 
Front left and right headlight LEDX2 

	Tail light 
	Brake light LEDX29 
Rear left and right headlight LEDX2 
Tail light  LEDX29



